# Output node

The Output node converts an applied map into a material. It uses the height to generate the normal and occlusion maps.

## Inputs

The Output node accepts the height, albedo, ORM, emission and normal channels of the applied map inputs.

## Outputs

The Output node outputs the albedo, metallic, roughness, emission, normal, occlusion and depth components of the material. They should be connected to the Material node.

## Parameters

The Output node accepts the following parameters:

- the amount of occlusion extracted from the height map

- the strength of the normal maps of the base material (when mixed with the normal map generated from the height map)