# Sixteen Segment Display node

The Sixteen Segment Display node outputs a sixteen segment display with variable weight

## Inputs

The Sixteen Segment Display node accepts an optional bevel map, which the parameter is multiplied by the map value.

## Outputs

The Sixteen Segment Display node outputs two grayscale images, the generated display and a hard mask for all segments

## Parameters

The Sixteen Segment Display node accepts the following parameters:

- The Display Mode parameter how the Character Code is handled. ASCII handles the Character Code as an ASCII code (32-115), where 31 displays all segments. Custom interprets the Character Code as an unsigned 16-bit integer(0-65535), where bit positions are used to determine which segments to be turned on.

- The Character Code parameter specifies the character to display, based on the Display Mode

- The Gap parameter specifies the distance between each segment on the display.

- The Thickness parameter controls the thickness of the segments.

- The DP Size parameter controls the size of the decimal point on the display.

- The DP Position parameter specifies the position of the decimal point on the display.

- The Diagonals Rotation parameter controls the rotation of the four diagonal segments on the display.

- The Bevel parameter controls the width of the edge of each segment.

- The Decimal Point parameter toggles the decimal point on the display on or off, when the Display Mode is set to Custom

## Example images